{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Sheet1","Sheet2"],"not_rendered":{"external_links":1,"defined_names":1,"comments":11},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":36,"n_cols":11,"rows_kept":36,"flags":["formulas_cached_only"]}
["类别","行政区","企业名称","监测点名称","执行标准名称","监测日期（yyyy/mm/dd）","监测项目名称","污染物浓度","标准限值","是否达标","超标倍数"]
["废水重点","高明区","佛山市法恩洁具有限公司","酸碱废水排放口（WS-15117-3)","《电镀水污染物排放标准》\n（DB 44/1597-2015）排放限值","2024-10-21","pH值",7.5,"6~9","是"]
["废水重点","高明区","佛山市法恩洁具有限公司","酸碱废水排放口（WS-15117-3)","《电镀水污染物排放标准》\n（DB 44/1597-2015）排放限值","2024-10-21","总氮",7.12,20,"是"]
["废水重点","高明区","佛山市法恩洁具有限公司","酸碱废水排放口（WS-15117-3)","《电镀水污染物排放标准》\n（DB 44/1597-2015）排放限值","2024-10-21","氨氮",0.648,15,"是"]
["废水重点","高明区","佛山市法恩洁具有限公司","酸碱废水排放口（WS-15117-3)","《电镀水污染物排放标准》\n（DB 44/1597-2015）排放限值","2024-10-21","化学需氧量",7,80,"是"]
["废水重点","高明区","佛山市法恩洁具有限公司","酸碱废水排放口（WS-15117-3)","《电镀水污染物排放标准》\n（DB 44/1597-2015）排放限值","2024-10-21","总磷",0.07,{"v":1,"d":"1.0"},"是"]
["废水重点","高明区","佛山市法恩洁具有限公司","酸碱废水排放口（WS-15117-3)","《电镀水污染物排放标准》\n（DB 44/1597-2015）排放限值","2024-10-21","悬浮物","4L",30,"是"]
["废水重点","高明区","佛山市法恩洁具有限公司","酸碱废水排放口（WS-15117-3)","《电镀水污染物排放标准》\n（DB 44/1597-2015）排放限值","2024-10-21","石油类",0.38,{"v":2,"d":"2.0"},"是"]
["废水重点","高明区","佛山市法恩洁具有限公司","酸碱废水排放口（WS-15117-3)","《电镀水污染物排放标准》\n（DB 44/1597-2015）排放限值","2024-10-21","六价铬","0.004L",0.1,"是"]
["废水重点","高明区","佛山市法恩洁具有限公司","酸碱废水排放口（WS-15117-3)","《电镀水污染物排放标准》\n（DB 44/1597-2015）排放限值","2024-10-21","总铬","0.03L",0.5,"是"]
["废水重点","高明区","佛山市法恩洁具有限公司","酸碱废水排放口（WS-15117-3)","《电镀水污染物排放标准》\n（DB 44/1597-2015）排放限值","2024-10-21","总铜","0.05L",0.5,"是"]
["废水重点","高明区","佛山市法恩洁具有限公司","酸碱废水排放口（WS-15117-3)","《电镀水污染物排放标准》\n（DB 44/1597-2015）排放限值","2024-10-21","总镍","0.01L",0.5,"是"]
["废水重点","高明区","佛山市法恩洁具有限公司","六价铬废水排放口（WS-15117-2)","《电镀水污染物排放标准》\n（DB 44/1597-2015）排放限值","2024-10-21","六价铬",0.006,0.1,"是"]
["废水重点","高明区","佛山市法恩洁具有限公司","总镍废水排放口（WS-15117-1)","《电镀水污染物排放标准》\n（DB 44/1597-2015）排放限值","2024-10-21","总镍",0.09,0.5,"是"]
["固定源废气VOCs","高明区","佛山市高明顺恒利塑胶有限公司","锅炉废气排放口（FQ-08027-1）","《锅炉大气污染物排放标准》（DB44/765-2019）标准限值","2024-10-16","颗粒物（烟/粉尘）","<20",20,"是"]
["固定源废气VOCs","高明区","佛山市高明顺恒利塑胶有限公司","锅炉废气排放口（FQ-08027-1）","《锅炉大气污染物排放标准》（DB44/765-2019）标准限值","2024-10-16","SO2","3L",50,"是"]
["固定源废气VOCs","高明区","佛山市高明顺恒利塑胶有限公司","锅炉废气排放口（FQ-08027-1）","《锅炉大气污染物排放标准》（DB44/765-2019）标准限值","2024-10-16","NOX",39,150,"是"]
["固定源废气VOCs","高明区","佛山市高明顺恒利塑胶有限公司","锅炉废气排放口（FQ-08027-1）","《锅炉大气污染物排放标准》（DB44/765-2019）标准限值","2024-10-16","烟气黑度","<1",1,"是"]
["固定源废气VOCs","高明区","佛山市高明顺恒利塑胶有限公司","表处理废气排放口（FQ-08027-6）","《合成革与人造革工业污染物排放标准》（GB 21902-2008）标准限值","2024-10-16","苯","0.01L","---","---"]
["固定源废气VOCs","高明区","佛山市高明顺恒利塑胶有限公司","表处理废气排放口（FQ-08027-6）","《合成革与人造革工业污染物排放标准》（GB 21902-2008）标准限值","2024-10-16","甲苯与二甲苯合计",0.04,"---","---"]
["固定源废气VOCs","高明区","佛山市高明顺恒利塑胶有限公司","表处理废气排放口（FQ-08027-6）","《合成革与人造革工业污染物排放标准》（GB 21902-2008）标准限值","2024-10-16","总VOCs",1.76,150,"是"]
["固定源废气VOCs","高明区","佛山市高明顺恒利塑胶有限公司","3#发泡炉\n废气排放口（FQ-08027-5）","《合成革与人造革工业污染物排放标准》（GB 21902-2008）标准限值","2024-10-16","苯","0.01L","---","---"]
["固定源废气VOCs","高明区","佛山市高明顺恒利塑胶有限公司","3#发泡炉\n废气排放口（FQ-08027-5）","《合成革与人造革工业污染物排放标准》（GB 21902-2008）标准限值","2024-10-16","甲苯与二甲苯合计",{"v":0.1,"d":"0.10"},"---","---"]
["固定源废气VOCs","高明区","佛山市高明顺恒利塑胶有限公司","3#发泡炉\n废气排放口（FQ-08027-5）","《合成革与人造革工业污染物排放标准》（GB 21902-2008）标准限值","2024-10-16","总VOCs",15.86,150,"是"]
["废气重点","高明区","佛山市高明区首邦化工有限公司","油性涂料车间（一车间）生产废气排放口（FQ-10305-1）","《涂料、油墨及胶粘剂工业大气污染物排放标准》（GB 37824-2019）排放限值","2024-10-24","非甲烷总烃",56.8,60,"是"]
["废水重点","高明区","广东睿鹏材料科学有限公司","废水排放口（DW001)","《合成树脂工业污染物排放标准》\n（GB 31572-2015）及《水污染物排放限值》（DB44/26-2001）排放限值","2024-10-28","悬浮物","4L",30,"是"]
["废水重点","高明区","广东睿鹏材料科学有限公司","废水排放口（DW001)","《合成树脂工业污染物排放标准》\n（GB 31572-2015）及《水污染物排放限值》（DB44/26-2001）排放限值","2024-10-28","化学需氧量",15,60,"是"]
["废水重点","高明区","广东睿鹏材料科学有限公司","废水排放口（DW001)","《合成树脂工业污染物排放标准》\n（GB 31572-2015）及《水污染物排放限值》（DB44/26-2001）排放限值","2024-10-28","氨氮",0.246,{"v":8,"d":"8.0"},"是"]
["废水重点","高明区","广东睿鹏材料科学有限公司","废水排放口（DW001)","《合成树脂工业污染物排放标准》\n（GB 31572-2015）及《水污染物排放限值》（DB44/26-2001）排放限值","2024-10-28","总磷",0.08,{"v":1,"d":"1.0"},"是"]
["废水重点","高明区","广东睿鹏材料科学有限公司","废水排放口（DW001)","《合成树脂工业污染物排放标准》\n（GB 31572-2015）及《水污染物排放限值》（DB44/26-2001）排放限值","2024-10-28","总氰化物",0.005,0.3,"是"]
["废水重点","高明区","广东睿鹏材料科学有限公司","废水排放口（DW001)","《合成树脂工业污染物排放标准》\n（GB 31572-2015）及《水污染物排放限值》（DB44/26-2001）排放限值","2024-10-28","pH值",6.9,"6~9","是"]
["废水重点","高明区","广东睿鹏材料科学有限公司","废水排放口（DW001)","《合成树脂工业污染物排放标准》\n（GB 31572-2015）及《水污染物排放限值》（DB44/26-2001）排放限值","2024-10-28","总氮",1.31,40,"是"]
["废水重点","高明区","广东睿鹏材料科学有限公司","废水排放口（DW001)","《合成树脂工业污染物排放标准》\n（GB 31572-2015）及《水污染物排放限值》（DB44/26-2001）排放限值","2024-10-28","五日生化需氧量",3.1,20,"是"]
["固定源废气VOCs","高明区","佛山市思贤家具有限公司","4楼底漆房有机废气排放口（FQ-17346-1）","《家具制造行业挥发性有机化合物排放标准》（DB44/814-2010）标准限值","2024-12-02","苯","0.01L",1,"是"]
["固定源废气VOCs","高明区","佛山市思贤家具有限公司","4楼底漆房有机废气排放口（FQ-17346-1）","《家具制造行业挥发性有机化合物排放标准》（DB44/814-2010）标准限值","2024-12-02","甲苯与二甲苯合计",0.13,20,"是"]
["固定源废气VOCs","高明区","佛山市思贤家具有限公司","4楼底漆房有机废气排放口（FQ-17346-1）","《家具制造行业挥发性有机化合物排放标准》（DB44/814-2010）标准限值","2024-12-02","总VOCs",0.57,30,"是"]

{"sheet":"Sheet2","index":1,"n_rows":11,"n_cols":10,"rows_kept":11,"flags":["formulas_cached_only"]}
["废气重点","废水重点","污水厂","危废企业废气","危废企业废水","重金属废气","重金属废水","垃圾场废水","垃圾场废气","垃圾场地下水"]
["废气重点"]
["废水重点"]
["污水厂"]
["危废企业废气"]
["危废企业废水"]
["重金属废气"]
["重金属废水"]
["垃圾场废水"]
["垃圾场废气"]
["垃圾场地下水"]